Table of contents
TECE sanitary modules
TECE sanitary modules
TECEprofil toilet module with Uni
cistern, installation height 1120 mm
Toilet module including “easy fit” flush
plate installation. For fitting to
TECEprofil section tubes or for
installation in metal or wooden stud
walls and as a pre-wall or corner module
also suitable for single block assembly.
Uni cistern for front actuation:
- Safety tank made of impact-resistant
plastic, tested to EN 14055
- Cistern fully pre-assembled and
sealed.
- Cistern connection with outer thread R
1/2” at the side, compatible with quick
adapters
- 10 litre tank volume 6 litre pre-set
standard flush volume, 4.5/7.5/9-litre
flush volume can be set at any time
3-litre partial flush volume for
dual-flush system remaining volume can
be used for immediate cleaning flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single or dual-flush
cistern
- “easy fit” flush plate installation
- Low-noise hydraulic filling valve,
fitting group 1 according to DIN 4109
Module frame:
- Self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 with joint
adapter DN 90/100, made of PP
- Joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90
A raised ceramic attachment for a
sitting height of 48 cm can be added in
keeping with German standard DIN 18040
(DIN 18040: Barrier-free construction -
Part 1: Publicly accessible buildings
and workplaces). Order-No.: 9300302