Table of contents
TECE sanitary modules
TECE sanitary modules
TECEconstruct toilet module with Uni
750-cistern, installation height 750 mm
Toilet module including “easy fit” flush
plate assembly. For single block
mounting, as a pre-wall module in front
of solid walls, and for incorporation
into metal or wooden stud walls.
Uni 750-cistern for actuation from
above:
- Safety tank made of impact-resistant
plastic, tested according to EN 14055
- Cistern fully pre-assembled and sealed
- Cistern connection with outer thread R
1/2” on the side
- 8-litre tank volume 6-litre pre-set
standard flush volume, 4.5-litre flush
volume can be set at any time 3-litre
partial flush volume for dual immediate
cleaning for dual-flush system residual
volume can be used for immediate
cleaning flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single-flush or
dual-flush cistern
- “easy fit” flush plate mounting
- Low-noise hydraulic filling valve,
acoustic group 1 according to DIN 4109
Module frame:
- self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 on DN 110,
made of PVC
- DN 90 toilet connection set including
protective plugs
- Mounting set for solid walls
Order-No.: 9300290