Oглавление
Застенные модули ТЕСЕ
Застенные модули ТЕСЕ
Застенный модуль TECEprofil со смывным
бачком Uni 750, высота 750 мм Toilet
module including “easy fit” flush plate
assembly. For fitting to TECEprofil
section tubes or for installation in
metal or wooden stud-and-beam walls and
as a pre-wall or corner module also
suitable for single block assembly.
Uni 750-cistern for actuation from
above:
- Safety tank made of impact-resistant
plastic, tested according to EN 14055
- Cistern fully pre-assembled and sealed
- Cistern connection with external
thread R 1/2” on the side, compatible
with quick adapters
- 8-litre tank volume 6-litre pre-set
standard flush volume, 4.5-litre flush
volume can be set at any time 3-litre
partial flush volume for dual immediate
cleaning for dual-flush system residual
volume can be used for immediate
cleaning flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single-flush or
dual-flush cistern
- “easy fit” flush plate mounting
- Installation tunnel for service
opening, can be shortened without tools
- Low-noise hydraulic filling valve,
acoustic group 1 according to DIN 4109
Module frame:
- self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 with joint
adapter DN 90/100, made of PP
- Joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90
- WC connection box including bare-wall
protection with junction box
A raised ceramic attachment for a
sitting height of 48 cm can be added in
keeping with German standard DIN 18040
(DIN 18040: Barrier-free construction -
Part 1: Publicly accessible buildings
and workplaces). Order-No.: 9300291