Table of contents
TECE sanitary modules
TECE sanitary modules
TECEprofil toilet module with Uni
750-cistern, installation height 750 mm
Toilet module including “easy fit” flush
plate assembly. For fitting to
TECEprofil section tubes or for
installation in metal or wooden
stud-and-beam walls and as a pre-wall or
corner module also suitable for single
block assembly.
Uni 750-cistern for actuation from
above:
- Safety tank made of impact-resistant
plastic, tested according to EN 14055
- Cistern fully pre-assembled and sealed
- Cistern connection with external
thread R 1/2” on the side, compatible
with quick adapters
- 8-litre tank volume 6-litre pre-set
standard flush volume, 4.5-litre flush
volume can be set at any time 3-litre
partial flush volume for dual immediate
cleaning for dual-flush system residual
volume can be used for immediate
cleaning flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single-flush or
dual-flush cistern
- “easy fit” flush plate mounting
- Installation tunnel for service
opening, can be shortened without tools
- Low-noise hydraulic filling valve,
acoustic group 1 according to DIN 4109
Module frame:
- self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 with joint
adapter DN 90/100, made of PP
- Joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90
- WC connection box including bare-wall
protection with junction box
A raised ceramic attachment for a
sitting height of 48 cm can be added in
keeping with German standard DIN 18040
(DIN 18040: Barrier-free construction -
Part 1: Publicly accessible buildings
and workplaces). Order-No.: 9300291