Table of contents
TECEfloor
TECEfloor
TECEfloor Standard RTL box Control unit
for decentralised individual room
temperature control including return
temperature limitation for floor and
wall heating systems in combination with
a radiator installation.
Consisting of:
- Shell set with wall installation box
with presettable control valve,
presettable RTL and thermostatic valve,
including bare-wall protection and
connection adapter 3/4” Eurocone,
installation depth: 65-90 mm.
- Fine installation set with plastic
cover plate in high-gloss white, shapely
thermostat control head and installation
frame
Order-No.: 77470005