Table of contents
TECE sanitary modules
TECE sanitary modules
TECEbase toilet module with Base 320
cistern, installation height 1120 mm
Toilet module for single block assembly,
suitable as a pre-wall module in front
of solid walls and for installation in
metal or wooden stud walls.
Base 320 cistern for operation from the
front:
- Safety tank made of impact-resistant
plastic, tested according to EN 14055
- Cistern completely pre-assembled
- Cistern connection with R 1/2” outer
thread from above, compatible with
quick-action adapters
- 3-way corner valve shut-off valve with
flush function when filling valve is
fitted
- 7 litre tank volume 6 litre preset
standard flush volume 4.5 litre flush
volume adjustable at any time 3 litre
partial flush with dual-flush system
setting of a 4/2 litre flush volume
optionally possible. Remaining volume
can be used for immediate cleaning
flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single or dual-flush
cistern
- Low-noise hydraulic filling valve,
acoustic group 1 according to DIN 4109
Module frame:
- self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 incl. joint
adapter DN 90/100 made of PP
- Joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90, including
building protection plug
- Mounting set for solid walls
Order No.: 9400440