Table of contents
TECEfloor
TECEfloor
TECEfloor SLQ PE- RT 5S BMB underfloor
heating pipe Five-layer underfloor
heating pipe in accordance with EN ISO
21003 made of high-density polyethylene
with higher temperature resistance
(PE-RT type 2). Oxygen-tight with
co-extruded EVOH coating to DIN 4726
application area Tmax 90 °C, 6 bar.
Suitable for particularly harsh
installation conditions thanks to the
5-layer technology SLQ quality-monitored
and compatibility tested.
DIN CERTCO 3V423 MVR (P)
Classification according to EN ISO
22391-2:
Application class 4 and 5: 6 bar, Tmax
90 °C
BMB at TECE stands for products based on
the biomass balance approach. Here,
biogenic raw materials (waste and
residual materials from biomass) are
used together with fossil raw materials
in the manufacture of basic chemical
products in the production network. The
bio content is then mathematically
allocated to the TECEfloor SLQ PE-RT 5S
BMB panel heating pipes on the basis of
the ISCC Plus certification system.
BMB products have the same quality as
non-BMB products, as the formulation of
the product is identical to that of the
fossil equivalent. TECE’s biomass
balance approach supports the use of
biogenic raw materials, which leads to
savings in fossil raw materials and a
reduction in greenhouse gas emissions.
Dimension: 16 x 2,0 mm Material: PE-RT
type II/EVOH/PE-RT type II Order No.:
77111635