Table of contents
TECE sanitary modules
TECE sanitary modules
TECEprofil toilet module with Uni
cistern, with integrated warm and cold
water hygiene flushing function,
installation height 1120 mm Toilet
module including “easy fit” flush plate
assembly. For fixing to TECEprofil
section tubes or for installation in
metal or wooden stud walls and as a
pre-wall or corner module also suitable
for single block assembly.
Uni cistern for operation from the
front:
- Cistern with integrated hygienic flush
- Completely pre-installed flushing unit
with hygienic flushing function
- Multi-way shut-off valves with
function for flushing the pipework
before commissioning
- Two cistern connections with outer
thread R 1/2” at the top, for flushing
hot and cold water pipes (2 x cold water
possible), compatible with quick-action
adapters
- Safety tank made of impact-resistant
plastic, tested to EN 14055
- Cistern completely pre-assembled and
sealed
- 10 litre tank volume 6 litres preset
standard flush volume 4.5/7.5/9 litres
flush volume adjustable at any time 3
litres partial flush with dual-flush
system residual volume can be used for
immediate cleaning flush.
- Insulated against condensation water
- Suitable for TECE flush plates and
toilet flush handles
- Can be used as a single or dual-flush
cistern
- “easy fit” flush plate installation
- Installation tunnel for service
opening, can be shortened without tools
- Low-noise hydraulic filling valve,
acoustic group 1 in accordance with DIN
4109
- Mains connection with transformer
including connection cable
- Fill level sensor, protects against
backflow in the cistern
- Flow control throttle without removing
the drain valve
Operation:
- Locally via Bluetooth interface via
TECE Smartconnect app
- Centralised and location-independent
via Ethernet or Wi-Fi interface via TECE
Smartconnect web application, optionally
via BMS interface
- Setting the flush intervals or flush
days in combination with the flush
volume
- Setting temperatures for
temperature-controlled flushing
- Flush history logging
Module frame:
- Self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drainage bend DN 90 with joint
adapter DN 90/100 made of PP
- joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90
- Toilet connection box including
rough-in protection, with junction box
and cover for transformer
Setting of a raised ceramic attachment
for 48 cm seat height, possible in
accordance with DIN 18040 (DIN 18040-1:
Construction of accessible buildings -
Design principles - Part 1: Publicly
accessible buildings).
Please order separately:
- TECE Gateway (item no. 9810013)
- Toilet flush plate (see flush plates)
- Fitting for pre-wall, corner or wooden
stud structures
- Power cable for building management
system (optional)
- TECE dry-wall construction upgrade set
for TECE shower toilets (optional)
Order No.: 9300104