Table of contents
TECE sanitary ceramics
TECE sanitary ceramics
TECEloft set, toilet ceramic with cyclon
flush, including seat/lid Set consists
of:
- TECEloft toilet ceramic with cyclon
flush
- TECEloft toilet seat/lid in classic
high design
- Concealed attachment
- Assembly instructions
Toilet ceramic features:
- Wall-mounted washdown toilet
- Flush water requirement: suitable for
flush water volumes of 4 and 2 litres
- Rimless, therefore no hidden areas for
deposits and dirt
- Cyclon flush technology (thorough and
quiet flushing thanks to ring-shaped
water flow inside the ceramic)
- Compact design – projection 515 mm
- Concealed wall attachment and
concealed water connection
- Material: Sanitary ceramic, colour
white
- Approved according to EN 997 type 1,
subtypes 6, 5 and 4
- Dimensions (W x H x D): 355 x 313 x
515 mm
Toilet seat features:
- Lid encloses seat
- Quick installation thanks to simple
clip-on design
- Easy to clean, complete seat and lid
unit removable
- Stainless steel hinges with soft-close
mechanism
- Made of torsion-resistant thermoset
plastic, colour: white
- Approved in accordance with DIN 19516
Order No.: 9700224